|  |  |
| --- | --- |
| **DUE PIN** | **BOARD FUNCTION** |
| Tx3 (14) | CAN\_INTERRUPT |
| 52 | CAN\_CHIPSELECT |
| MISO | MCP2515 MISO |
| MOSI | MCP2515 MOSI |
| SCK | MCP2515 SCK (CLOCK) |
| A4 | STATE\_OUT HEAD LIGHTS |
| A5 | STATE\_OUT HAZARD |
| A6 | STATE\_OUT BRAKE |
| A7 | STATE\_OUT STROBE |
| A8 | Horn |
| A9 | Left Turn |
| A10 | Right Turn |
|  |  |
|  |  |
|  |  |
|  |  |